Several rectifiers can be connected in parallel to obtain higher output current, but they must be equipped with the parallel configuration option. **NOTE** that if more than one rectifier stack shall be connected in parallel then each stacks bus bar shall be connected together with the other stacks DC outputs. Please see Figure 5 Three rectifier stacks connected in parallel.

### Blocking the rectifier RUN/BLOCK

The rectifier can be blocked and stopped without entering “STANDBY”.

The blocking function turns the rectifier output off and it restarts with the set values. In DUAL-2 mode output A and B are blocked independently.

This can be done using the “BLOCK” key, from the main menu, from the SET menu, or by remote control. In DUAL-2 mode the rectifiers can only be operated independently from the SET menu, or by remote control.